{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Munka1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Munka1","index":0,"n_rows":15,"n_cols":2,"rows_kept":15,"cut":false,"hidden":false,"merged":[]}
["Csecsemőkori hallásszűrő"]
[]
["Vizsgálójel a mérés során BERA esetén","Chirp"]
["Vizsgáló intenzitás BERA esetén","min. 25 dBHL"]
["Vizsgálati időtartam BERA esetén","max. 3 perc"]
["Alacsony műtermékszint","max. 100 μV"]
["Kiegészítő szűrőfunkciók","DPOAE és TEOAE"]
["Többszínű jelzőfény","ellenállás és vizsgálat előrehaladtának jelzése"]
["Fogyóeszköz biztosítása","Minimum 3 évnyi fogyóeszköz biztosítása (kb. 350 mérés / év)"]
["Bőr impedancia mérés","automatikus"]
["Szűrő BERA funkció","gyors és automatizált"]
["Rendszer kialakítás (fejmérethez )","szabályozható"]
["Kijelző","nagyobb min 4\"-os érintőképernyő"]
["Pc kompatibilitás","Saját szoftverrel vagy Noah rendszerrel kommunikál"]
["Áramforrás","tölthető Li-ion akkumulátor"]