{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Munka1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Munka1","index":0,"n_rows":2,"n_cols":4,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
["A termék megnevezése","Műszaki paraméterek","Igényelt mennyiség","A gyártó megnevezése"]
["Fecskendő pumpa","4 fecskendő különálló vezérlésére képes, érintőképernyővel vezérelhető, programozható fecskendőpumpa, vagy fecskendő pumpa rendszer.  A fecskendők esetében külön állítható legyen az adagolás/visszaszívás iránya és sebessége.\nMin fecskendőméret: 10-ul-60 mL, vagy szélesebb tartományban változtatható legyen. Az adagolás sebessége min. 0.184nL/min～83.318mL/min, vagy szélesebb áramlási tartományban változtatható legyen (a min.-max. fecskendőméret figyelembe vételével.Lehetőség szerint  USB és RS232 kimenettel egyaránt rendelkezzen. ","1 db","LeadFluid TFD04/4*ZX02 vagy KDS GEMINI 88 PLUS"]