{"text_format":"2","workbook":"xlsx","n_sheets":22,"sheets":["Terméklista","Labortáp","Diff probe","Forrasztóállomás","Pákahegy","Hőlégfúvó","Multiméter","Multiméter kiegészítő","STM32 programozó","FPGA programozó debug","Blankoló","Ultrasonic Cleaner","Csipesz készlet","Dremel szerszámkészlet","Csupaszoló","Csavarhúzó készlet","Kaparó","Dremel motor","Proxxon micro furóállvány","Proxxon micro eszterga","CIF csendes kompresszor ","Molex crimpelő fogó"],"not_rendered":{"charts":0,"images":4,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Terméklista","index":0,"n_rows":31,"n_cols":5,"rows_kept":31,"cut":false,"hidden":false,"merged":[[28,1,28,3],[29,1,29,3],[30,1,30,3]]}
["#","Megnevezés","Igényelt mennyiség (db)","Típus","Elfogadott helyettesítő termék"]
[1,"Labortáp",1,"EX354RT -  Bench Power Supply, Mixed Mode Regulated, Adjustable, 3 Output, 0 V, 35 V, 0 A, 4 A"]
[{"$f":"A2+1","v":2},"Diff probe",1,"TA045 -  Oscilloscope Probe, Differential, 200 MHz, 60 V, 10:1, All Makes & Models of Oscilloscopes","TT-SI 9101 -  Oscilloscope Probe, Differential, 100 MHz, 700 V, 10:1, 100:1, All Makes & Models of Oscilloscopes"]
[{"$f":"A3+1","v":3},"Forrasztóállomás",2,"Ersa I-CON1 -  80W Soldering Station"]
[4,"Pákahegy",2,"0102PDLF07/SB -  Soldering Iron Tip, Pencil, 0.7 mm"]
[5,"Pákahegy",2,"0102PDLF02/SB -  Soldering Iron Tip, Pencil, 0.2 mm"]
[6,"Pákahegy",2,"0102PDLF04/SB -  Soldering Iron Tip, Pencil, 0.4 mm"]
[7,"Pákahegy",2,"0102CDLF12/SB -  Soldering Iron Tip, Chisel, 1.2 mm"]
[8,"Hőlégfúvó",1," WTHA 1 -  Soldering Station, Hot Air, 230 V, 900 W, 600°C Max Temperature, EU/UK Plug "]
[9,"Multiméter",1,"FLUKE 289/EUR -  Industrial Multimeter, Fluke 289 Series, 50000 Count, True RMS, Auto, Manual Range, 4.5 Digit"]
[10,"Multiméter kiegészítő",1," FLUKE IR3000FC -  Test Accessory, DMM & Processmeter, Wireless Data Transfer Connector "]
[11,"STM32 programozó",4,"ST-LINK/V2 -  In Circuit Debugger/Programmer, For STM8 & STM32, SWIM and JTAG Serial Wire Debugging Interfaces"]
[12,"FPGA programozó/debug",1,"HW-USB-II-G -  Programmer, Platform Cable USB II, In-Circuit, Xilinx FPGA/PROM Devices, USB"]
[13,"Blankoló",1,"STRIPAX -  Wire Stripper, STRIPAX, 28-10 AWG / 0.8-6mm² Capacity PVC Insulation Cables"]
[14,"Ultrasonic Cleaner",1," UT8021/EUK -  Cleaning Tank, Ultrasonic, 2 L, 40 KHZ, 100 W, 150 mm x 100 mm x 137 mm "]
[15,"Csipeszkészlet",3,"18480EZ -  Tweezers Set, 6 Piece, E-Z Pik, with Pouch "]
[16,"Dremel szerszámkészlet",3,"2615E725JA -  Assorted Tool Set, 70 Pieces "]
[17,"Csupaszoló",2,"11476 -  3 Piece Mini Electrical Tool Set with Cutters, Crimpers and Strippers "]
[18,"Csavarhúzó készlet",2,"26199 -  SCREWDRIVER SET "]
[19,"Kaparó",2,"35630 -  PROBE KIT, 4 PIECES "]
[20,"Dremel motor",2,"F0134000KF -  Rotary Tool Kit, 35000 rpm, 175 W, 230 V "]
[21,"Proxxon micro fúróállvány",1," MF 70 -  Micro Miller, 240V, 100W, 20000 RPM, EU Plug "]
[22,"Proxxon micro fúróállvány",1," FF 230 -  Micro Miller, 230V, 140W, 2200 RPM "]
[23,"Proxxon micro eszterga",1,"FD 150/E -  Precision Lathe, Metal Working, Electronic Control, 360mm x 150mm x 150mm, 4.5KG "]
[24,"CIF csendes kompresszor ",1,"F41045 -  Silent Compressor, 17 Litres/min, 230V, 135W, 6bar, 30dB "]
[25,"Molex crimpelő fogó",1," 200218-2200 -  Crimp Tool, Ratchet, Molex Mini-Fit Jr. Series 16AWG Pin & Socket Contacts, 207129 Series "]
[26,"Molex crimpelő fogó",1,"63819-1500 -  Crimp Tool, Ratchet, Molex Pico-Clasp 501193 & 501334 Series 32-28AWG Contacts "]
[]
[null,"A kiírt tételekre csak együttes ajánlat tehető. "]
[null,"A kiajánlott árnak tartalmaznia kell minden járulékos költséget, az ajánlatkérő részajánlatot nem értékel, ajánlattevőnek minden, a felhívásban részletezett termékre és tartozékra ajánlatot kell adnia."]
[null,"Az ajánlati árnak tartalmaznia kell az összes adó, illeték, szállítási vagy egyéb járulékos költségeket is, a hatályos magyar jogszabályok szerint."]

{"sheet":"Labortáp","index":1,"n_rows":5,"n_cols":2,"rows_kept":5,"cut":false,"hidden":false,"merged":[[4,0,4,7]]}
["EX354RT -  Bench Power Supply, Mixed Mode Regulated, Adjustable, 3 Output, 0 V, 35 V, 0 A, 4 A"]
["Gyártó:","AIM-TTI INSTRUMENTS"]
["Gyártói cikkszám: ","EX354RT"]
[]
["By adding four digit meters and switchable remote sensing, the EX-R series offers much higher precision whilst retaining the simplicity of operation which many bench-top power supply users prefer. Six models are offered including single, dual and triple outputs and covering a power range of 175 watts up to 420 watts. The EX354RT incorporates a third output fully variable between 1.5V and 5.0V with a fixed current limit of 5A. The set voltage can be measured at the press of a button using the digital meters.                                                                                                                                                                                                                                                         - Triple output (2 x 0 to 35V / 0 to 4A plus 1.5 to 5.0V @ 5A)              \n- Independent digital voltage and current meters for each output with 4 digit resolution\n- Switchable local or remote sensing\n- Constant voltage or constant current operation\n- Variable 1.5 - 5.0V auxiliary output at 5A (EX354RT)\n- Compact design uses less bench space\n- Silent fan-free cooling\n- DC output switches, automatic mode indication\n"]

{"sheet":"Diff probe","index":2,"n_rows":5,"n_cols":10,"rows_kept":5,"cut":false,"hidden":false,"merged":[[4,0,4,5]]}
["TA045 -  Oscilloscope Probe, Differential, 200 MHz, 60 V, 10:1, All Makes & Models of Oscilloscopes",{"$nulls":7},"Helyettesítő termék ","TT-SI 9101 -  Oscilloscope Probe, Differential, 100 MHz, 700 V, 10:1, 100:1, All Makes & Models of Oscilloscopes"]
["Gyártó:","PICO TECHNOLOGY",{"$nulls":6},"Gyártó","TESTEC"]
["Gyártói cikkszám: ","TA045",{"$nulls":6},"Gyártói cikkszám:","TT-SI 9101"]
[]
["The TA045 is a Differential Probe enables conventional oscilloscopes to display and measure in-circuit waveforms that are referenced to high common-mode voltages, this differential probe extends the measurement capability of oscilloscopes to digital communications and high-speed digital circuits. It complies with IEC-1010.1, IEC-1010.2-031 CAT I and pollution degree 2.\n- 500kR/7pF Each side to ground input impedance\n- 50R Source impedance (typical)\n- Additional power supply or battery pack is required",{"$nulls":7},"Oscilloscope Probe Function: Differential  Bandwidth: 100MHz  \nInput Voltage Max: 700V  \nTest Probe Attenuation: 10:1, 100:1  \nFor Use With: All Makes & Models of Oscilloscopes  \nProduct Range: -"]

{"sheet":"Forrasztóállomás","index":3,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
["Ersa I-CON1 -  80W Soldering Station"]
["Gyártó:","ERSA"]
["Gyártói cikkszám: ","I-CON1"]
[]
["dimensions (W x D x H)","150 x 175 x 105 mm "]
[" weight","3,0 kg i-CON 1 V / 3,7 kg i-CON 2V"]
[" voltage","  230 V AC, 50 Hz"]
["nominal power "," 80 W i-CON 1 V / 120 W i-CON 2V"]
[" design"," antistatic "]
["temperature range ","50 – 450 °C"]
["Comaptible with the following soldering tips:","0102CDLF12/SB; 0102PDLF04/SB"]

{"sheet":"Pákahegy","index":4,"n_rows":16,"n_cols":2,"rows_kept":16,"cut":false,"hidden":false,"merged":[[7,0,7,4],[3,0,3,12],[11,0,11,12],[15,0,15,12]]}
["0102PDLF07/SB -  Soldering Iron Tip, Pencil, 0.7 mm"]
["Gyártó:","ERSA"]
["Gyártói cikkszám: "," 0102PDLF07/SB"]
["The 0102PDLF07/SB is a 0.7mm long-life chisel-shaped Soldering Tip with ERSADUR-LF coating for i-Tool soldering iron for i-CON soldering station."]
[]
["0102PDLF02/SB -  Soldering Iron Tip, Pencil, 0.2 mm"]
["Gyártói cikkszám: ","0102PDLF02/SB"]
["The 0102PDLF02/SB is a pencil point Soldering Tip and lead-free soldering will require higher working temperatures. In addition, the higher tin (Sn) content in the lead-free solder will greatly increase the stress degradation to the solder tip, thereby decreasing the life of the tip considerably. In order to increase the tip life, soldering tip manufacturers must adjust the amount of iron (Fe) plating on the tips. The base material made of highly conductive electrolytic copper ensures unhindered heat transfer from the heating element to the ERSADUR-LF coating."]
[]
["0102PDLF04/SB -  Soldering Iron Tip, Pencil, 0.4 mm"]
["Gyártói cikkszám: ","0102PDLF04/SB"]
["The 0102PDLF04/SB is a 0.4mm long-life chisel-shaped Soldering Tip with ERSADUR-LF coating for i-Tool soldering iron for i-CON soldering station."]
[]
["0102CDLF12/SB -  Soldering Iron Tip, Chisel, 1.2 mm"]
["Gyártói cikkszám: ","0102CDLF12/SB"]
["The 0102CDLF12/SB is a 1.2mm long-life chisel-shaped Soldering Tip with ERSADUR-LF coating for i-Tool soldering iron for i-CON soldering station."]

{"sheet":"Hőlégfúvó","index":5,"n_rows":12,"n_cols":2,"rows_kept":12,"cut":false,"hidden":false,"merged":[]}
[" WTHA 1 -  Soldering Station, Hot Air, 230 V, 900 W, 600°C Max Temperature, EU/UK Plug "]
["Gyártó:"," WELLER"]
["Gyártói cikkszám: ","WTHA 1"]
[]
["Dimensions L x W x H: ","210 x 160 x 125 mm 8.30 x 6.30 x 4.90 in     "]
["Fuse: ","120 V (A) T8 A"]
[" Weight: ","3.0 kg / 6.6 lbs"]
["Power supply: ","120 V / 60 Hz"]
["Power consumption: ","900 W"]
["ESD: ","safe Yes"]
["Temperature range (expanded hot air) l/min 100: ","50 °C – 600 °C 120 °F – 1100 °F "]
["Temperature accuracy:"," ± 30 °C / ± 54 °F"]

{"sheet":"Multiméter","index":6,"n_rows":15,"n_cols":2,"rows_kept":15,"cut":false,"hidden":false,"merged":[]}
["FLUKE 289/EUR -  Industrial Multimeter, Fluke 289 Series, 50000 Count, True RMS, Auto, Manual Range, 4.5 Digit"]
["Gyártó:","FLUKE "]
["Gyártói cikkszám: ","FLUKE 289/EUR"]
[]
["Maximum voltage between any terminal and earth ground: 1000 V      "]
["Battery type: ","6 AA alkaline batteries, NEDA 15A IEC LR6"]
["Battery life: ","100 hours minimum, 200 hours in logging mode"]
["Temperature: ","Operating: -20 °C to 55 °C"]
[" Storage:"," -40 °C to 60 °C "]
["Relative humidity: ","0 to 90 % (0 t 37 °C), 0 to 65 % (37 °C to 45 °C), 0 to 45 % (45 °C to 55 °C) "]
["Electromagnetic compatibility: ","EMC EN61326-1 "]
["Vibration: ","Random vibration per MIL-PRF-28800F Class 2"]
["Shock: ","1 meter drop per IEC/EN 61010-1 2nd Edition"]
["Size (HxWxL):"," 22.2 cm x 10.2 cm x 6 cm (8.75 in x 4.03 in x 2.38 in)"]
["Weight: ","870.9 g (28 oz)"]

{"sheet":"Multiméter kiegészítő","index":7,"n_rows":14,"n_cols":2,"rows_kept":14,"cut":false,"hidden":false,"merged":[]}
[" FLUKE IR3000FC -  Test Accessory, DMM & Processmeter, Wireless Data Transfer Connector "]
["Gyártó:","FLUKE"]
["Gyártói cikkszám: ","FLUKE IR3000FC"]
[]
["Battery type:","Two AAA Alkaline batteries, ANSI-24A IEC-LR03   "]
["Battery life: ","6 hours of continuous transmission"]
["RF communications: ","2.4 GHz ISM Band"]
["RF communication range: ","Open air, unobstructed: Up to 20 m Obstructed, sheetrock wall: Up to 6.5 m Obstructed, concrete wall or steel electrical enclosure: Up to 3.5 m "]
["Temperature: ","Operating: -10 °C to 50 °C ,  Storage: -20 °C to 60 °C "]
[" Certifications: ","CSA, FCC, CE, IC "]
["Warranty: ","Three years "]
["Weight: ","80 g "]
["Size: (HxWxL) ","3.2 cm x 7.6 cm x 6.4 cm (1.25 in x 3.0 in x 2.5 in)"]
["Compatibility: ","Fluke 187, 189, 287, 289, 789"]

{"sheet":"STM32 programozó","index":8,"n_rows":5,"n_cols":2,"rows_kept":5,"cut":false,"hidden":false,"merged":[[4,0,4,7]]}
["ST-LINK/V2 -  In Circuit Debugger/Programmer, For STM8 & STM32, SWIM and JTAG Serial Wire Debugging Interfaces"]
["Gyártó:","STMICROELECTRONICS"]
["Gyártói cikkszám: ","ST-LINK/V2"]
[]
["ST-LINK/V2 is an in-circuit debugger and programmer for the STM8 and STM32 microcontroller families. The single wire interface module (SWIM) and JTAG/serial wire debugging (SWD) interfaces are used to communicate with any STM8 or STM32 microcontroller located on an application board. STM8 applications use the USB full speed interface to communicate with ST Visual Develop (STVD) or ST Visual Program (STVP) software. STM32 applications use the USB full speed interface to communicate with Atollic, IAR, Keil or TASKING integrated development environments."]

{"sheet":"FPGA programozó debug","index":9,"n_rows":5,"n_cols":2,"rows_kept":5,"cut":false,"hidden":false,"merged":[[4,0,4,7]]}
["HW-USB-II-G -  Programmer, Platform Cable USB II, In-Circuit, Xilinx FPGA/PROM Devices, USB"]
["Gyártó:","XILINX"]
["Gyártói cikkszám: ","HW-USB-II-G"]
[]
["Xilinx is now offering its second generation Pb-Free (RoHS compliant) USB compatible cable for in-circuit configuration and programming of all Xilinx devices. The Platform Cable USB II provides integrated firmware to deliver high-performance, reliable and user-friendly configuration of Xilinx FPGAs and programming of Xilinx PROM and CPLD devices. The Platform Cable USB II cable optimizes direct programming of third-party SPI flash memory devices and indirect programming of SPI or parallel NOR flash memory devices via the FPGA JTAG port. In addition, Platform Cable USB II is a cost effective tool for debugging embedded software and firmware when used with Xilinx applications such as the Embedded Development Kit and ChipScope™ Pro Analyzer. Platform Cable USB II is an upgrade to and backwards compatible with Platform Cable USB. It has industry-leading performance and is compatible with Full Speed (USB 1.1) and Hi-Speed (USB 2.0) ports."]

{"sheet":"Blankoló","index":10,"n_rows":10,"n_cols":2,"rows_kept":10,"cut":false,"hidden":false,"merged":[[9,0,9,5]]}
["STRIPAX -  Wire Stripper, STRIPAX, 28-10 AWG / 0.8-6mm² Capacity PVC Insulation Cables"]
["Gyártó:","WEIDMULLER"]
["Gyártói cikkszám: ","STRIPAX"]
[]
["Stripping Capacity AWG: ","28AWG to 7AWG "]
["Stripping Capacity Metric: ","0.08mm² to 10mm²"]
["For Use With: ","Flexible & Solid Conductors "]
["Product Range: ","Stripax Series"]
[]
["The 9005000000 is a 7.48-inch STRIPAX Stripping and Cutting Tool with automatic self-adjustment for flexible and solid conductors with PVC insulation. Automatic opening of clamping jaws after stripping. Stripping length adjustable via end stop. Double-insulated cables in two process steps without special adjustment. Ideally suitable for mechanical and plant engineering, railway and rail traffic, wind energy, robot technology, explosion protection as well as marine, offshore and ship building sectors. "]

{"sheet":"Ultrasonic Cleaner","index":11,"n_rows":10,"n_cols":2,"rows_kept":10,"cut":false,"hidden":false,"merged":[]}
[" UT8021/EUK -  Cleaning Tank, Ultrasonic, 2 L, 40 KHZ, 100 W, 150 mm x 100 mm x 137 mm "]
["Gyártó:","SHESTO"]
["Gyártói cikkszám: ","UT8021/EUK"]
[]
["Capacity:  ","2l     "]
["Frequency: ","40kHz"]
["Power Consumption: ","100W"]
["External Height: ","100mm"]
["External Width:"," 137mm"]
["External Depth: ","150mm"]

{"sheet":"Csipesz készlet","index":12,"n_rows":14,"n_cols":2,"rows_kept":14,"cut":false,"hidden":false,"merged":[]}
["18480EZ -  Tweezers Set, 6 Piece, E-Z Pik, with Pouch "]
["Gyártó:","AVEN"]
["Gyártói cikkszám: ","18480EZ"]
[]
["Contains:","- 18013EZ, E-Z Pik Style AA Tweezers"]
[null,"- 18032EZ, E-Z Pik Style OO Tweezers"]
[null,"- 18049EZ, E-Z Pik Style 2A Tweezers"]
[null,"- 18056EZ, E-Z Pik Style 3C Tweezers"]
[null,"- 18062EZ, E-Z Pik Style #5 Tweezers"]
[null,"- 18072EZ, E-Z Pik Style #7 Tweezers"]
[]
["Material:","Stainless steel"]
["No. Of pieces:",6]
["Weight:","0.35 lb"]

{"sheet":"Dremel szerszámkészlet","index":13,"n_rows":5,"n_cols":2,"rows_kept":5,"cut":false,"hidden":false,"merged":[[4,0,4,7]]}
["2615E725JA -  Assorted Tool Set, 70 Pieces "]
["Gyártó:","DREMEL"]
["Gyártói cikkszám: ","2615E725JA"]
[]
["The 2615E725JA from Dremel is an EZ SpeedClic multipurpose accessory set. The Set contains 70 high quality genuine EZ SpeedClic accessories which allow for quick, easy and keyless accessory changes. EZ SpeedClic is Dremel's unique quick change system for rotary tool accessories. With this accessory set one can tackle a wide range of applications like cutting, sanding, grinding, polishing in a variety of different materials. The storage case allows to conveniently store Dremel accessories."]

{"sheet":"Csupaszoló","index":14,"n_rows":12,"n_cols":2,"rows_kept":12,"cut":false,"hidden":false,"merged":[[11,0,11,4],[6,0,6,4],[4,0,4,4],[5,0,5,4],[7,0,7,4],[8,0,8,4],[9,0,9,4],[10,0,10,4]]}
["11476 -  3 Piece Mini Electrical Tool Set with Cutters, Crimpers and Strippers "]
["Gyártó:","TITAN"]
["Gyártói cikkszám: ",11476]
[]
["Set includes: Cutter, Stripper, Crimper"]
["Cutting capacity: 30-10 Awg"]
["Stripping capacity: 22-10 Awg"]
["Crimping capacity: instulated terminals from 22-10 Awg"]
["Overall length og tools: 5- 1/2\""]
["For hard to reach applications"]
["Soring loaded to reduce fatigue"]
["Comfortable TPR handles for maximum grip"]

{"sheet":"Csavarhúzó készlet","index":15,"n_rows":5,"n_cols":2,"rows_kept":5,"cut":false,"hidden":false,"merged":[]}
["26199 -  SCREWDRIVER SET "]
["Gyártó:","WIHA"]
["Gyártói cikkszám: ",26199]
[]
["8-Pcs of 4 Slotted, 4 Phillips Screwdrivers"]

{"sheet":"Kaparó","index":16,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":false,"merged":[[9,0,9,6],[10,0,10,6],[4,0,4,6],[5,0,5,6],[6,0,6,6],[7,0,7,6],[8,0,8,6]]}
["35630 -  PROBE KIT, 4 PIECES "]
["Gyártó:","MENDA"]
["Gyártói cikkszám: ",35630]
[]
["Material: 300 Series Stainless Steel     "]
["Handle: 5/32\" (4mm) hex shape to prevent rolling"]
["Points: Semi hardened - may be reshaped for special applications as required"]
[" Item 35122: Straight needle point"]
["Item 35123: hook needle point"]
["Item 35617: Angle needle point"]
["Item 35623: Curved needle point"]

{"sheet":"Dremel motor","index":17,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":false,"merged":[]}
["F0134000KF -  Rotary Tool Kit, 35000 rpm, 175 W, 230 V "]
["Gyártó:","DREMEL"]
["Gyártói cikkszám: ","F0134000KF"]
[]
["Rated power input: 175 W      "]
["Voltage: 230 V"]
["Weight: 0,66 kg"]
["Length: 23 cm"]
["Width: 4.1 cm"]
["Depth: 4.3 cm"]
["No load speed: 5.000 - 35.000 1/min "]
[" Battery technology: n.a."]
[" Speed setting: Fully Variable"]
[" Accessory quick change system: EZ Twist "]
[" Sound pressure: 77,9 dB(A)"]
["Sound power: 88,9 dB(A)"]
["Vibration: 2,6 - 11,4 m/s²"]

{"sheet":"Proxxon micro furóállvány","index":18,"n_rows":16,"n_cols":2,"rows_kept":16,"cut":false,"hidden":false,"merged":[[15,0,15,7],[7,0,7,7]]}
[" MF 70 -  Micro Miller, 240V, 100W, 20000 RPM, EU Plug "]
["Gyártó:","PROXXON"]
["Gyártói cikkszám: ","MF 70"]
["Supply Voltage V AC: 240V "]
[" Input Power: 100W "]
["Spindle Speed: 20000 rpm"]
["Plug Type: EU"]
["230V, 100W, 50/60Hz. Spindle speeds 5,000 - 20,000rpm. Table 200 x 70mm with X-Y travel of 134 and 46mm respectively, with vertical travel 80mm. Footprint size 130 x 225mm and overall height 370mm. Weight approx. 7kg. The clamping blocks depicted are included too, but not the workpiece!"]
[]
[" FF 230 -  Micro Miller, 230V, 140W, 2200 RPM "]
["Gyártói cikkszám: FF 230"]
[]
["Supply Voltage V AC: 230V "]
[" Input Power: 140W "]
["Spindle Speed: 2200 rpm"]
["220 – 240V. 140W. 50/60Hz. Spindle speeds of 280 –\n550 – 870 – 1,200 – 1,500 and 2,200rpm. 30mm travel.\nTable size 270 x 80mm, column 35 x 400mm long. X-Ytravel is 170 x 65mm. Maximum height 180mm and\ndepth 130mm. Overall height approx. 500mm. Weight\napprox. 17kg."]

{"sheet":"Proxxon micro eszterga","index":19,"n_rows":5,"n_cols":2,"rows_kept":5,"cut":false,"hidden":false,"merged":[[4,0,4,7]]}
["FD 150/E -  Precision Lathe, Metal Working, Electronic Control, 360mm x 150mm x 150mm, 4.5KG "]
["Gyártó:","PROXXON"]
["Gyártói cikkszám: ","FD 150/E"]
[]
["220 – 240V. 50/60Hz. Distance between centres 150mm. Swing 55mm. Height over cross slide 33mm. Cross slide travel (X) 40mm, top slide travel (Z) 60mm. Steel tool post for turning steels 6 x 6mm. Spindle bore 8.5mm. 2-stage belt drive with electronic speed control: Stage 1 = 800 – 2,800rpm. Stage 2 = 1,500 – 5,000rpm. Dimensions approx. 360 x 150 x 150mm. Weight 4.5kg. Insulated to class 1."]

{"sheet":"CIF csendes kompresszor ","index":20,"n_rows":12,"n_cols":2,"rows_kept":12,"cut":false,"hidden":false,"merged":[]}
["F41045 -  Silent Compressor, 17 Litres/min, 230V, 135W, 6bar, 30dB "]
["Gyártó:","CIF"]
["Gyártói cikkszám: ","F41045"]
[]
["Power supply: 220 V AC, 50/60 Hz    "]
["Power: 135 W"]
[" Capacity: 1 litre"]
[" Production: 25 litres / min"]
["Max. pressure: 6 bars"]
["Sound level: 30 dB"]
["Net weight: 12 Kg "]
["Dimensions: 21 x 46 x 53 cm"]

{"sheet":"Molex crimpelő fogó","index":21,"n_rows":14,"n_cols":2,"rows_kept":14,"cut":false,"hidden":false,"merged":[[12,0,12,7],[13,0,13,7],[3,0,3,7],[8,0,8,7],[9,0,9,7],[10,0,10,7],[11,0,11,7]]}
[" 200218-2200 -  Crimp Tool, Ratchet, Molex Mini-Fit Jr. Series 16AWG Pin & Socket Contacts, 207129 Series "]
["Gyártó:","MOLEX"]
["Gyártói cikkszám: ","200218-2200"]
["A full cycle ratcheting hand tool ensures complete crimps. Ergonomic soft grip handles for comfortable crimping. A precision, user-friendly terminal locator wire stop holds terminals in the proper crimping position. Right- and left-handed applications. Dies and locator from this tool can be used in the Battery Powered Tool Order No. 63816-0200 (110 V) or 63816-0250 (220 V), with the use of the 63816-0800 Crimp Head. Many different tool kits can be used with a single Battery Powered Crimp Tool. This tool is IPC/WHMA-A-620 Class 2 compliant. This tool is RoHS compliant; however, RoHS compliance is not required"]
[]
[]
["63819-1500 -  Crimp Tool, Ratchet, Molex Pico-Clasp 501193 & 501334 Series 32-28AWG Contacts "]
["Gyártói cikkszám: ","63819-1500"]
["A full cycle ratcheting hand tool ensures complete crimps"]
["Ergonomic soft grip handles for comfortable crimping"]
["A precision user-friendly terminal locator wire stop holds terminals in proper crimping position"]
["Right and left handed applications"]
["Tool is WHMA-IPCA620 Class 2 compliant as indicated"]
["For 1.00mm (.039\") pitch Pico-Clasp™ wire-to-board crimp terminal, 28-32AWG"]