{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Munka1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Munka1","index":0,"n_rows":13,"n_cols":9,"rows_kept":13,"cut":false,"hidden":false,"merged":[]}
[null,null,"Specification for Call for Proposals # SZTE/2024/PB13690"]
[]
[null,"#","Description","Connection 1","Connection 2","Tube diameter","Design pressure","Reference: Swagelok part number","Quantity"]
[null,1,"Stainless steel relief valve with spring","NPT 1/4\"","NPT 1/4\"","1/4\"","PN8","SS-RL3M4-F4",1]
[null,2,"Stainless steel relief valve with spring","NPT 1/2\"","NPT 1/2\"","1/2\"","PN16","SS-RL4M8F8",3]
[null,3,"Stainless steel relief valve","NPT 1/2\"","NPT 1/2\"","1/2\"","PN16","SS-R4M8F8",2]
[null,4,"Relief valve spring; 16 bar","-","-","-","-","177-13K-R4-A",2]
[null,5,"Shipping , handling costs for the items above"]
[null,null,"Total net sum of the above"]
[]
[]
[]
[null,null,"Version date: February 20, 2024."]