{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":19,"n_cols":5,"rows_kept":19,"cut":false,"hidden":false,"merged":[]}
["Ssz.","Megnevezés","Mennyiség","Kiszerelés","Kompatibilitás"]
[1,"Filter Adapters for Syringes, A Ø 34 mm , PTFE","1 x","1 db","N 1666-16; BOLA"]
[2,"Tubing, Ø 0,8 x Ø 1,6 mm , FEP ","5 x","1 m","S 1815-04 (5 m); BOLA"]
[3,"Connection Bolts, UNF 10-32G, Ø 1,6 mm , PEEK","10 x","1 db","F 836-10; BOLA"]
[4,"Capillary Tubing, Ø 1/16\"(1,57 mm) x Ø 0,50 , PEEK","3 x","1 m","S 1817-12 (3 m); BOLA"]
[5,"Capillary Tubing, Ø 1/16\"(1,57 mm) x Ø 0,76 , PEEK","3 x","1 m","S 1817-16 (3 m); BOLA"]
[6,"Double Sealing Cones for Connection Bolts, UNF 10-32G, Ø 1,6 mm, PEEK","10 x","1 db","F 837-10; BOLA"]
[7,"Sealing Cones for Connection Bolts; UNF 10-32G, Ø 1,6 mm , PEEK","10 x","1 db","F 834-10; BOLA"]
[8,"Connection Bolts; UNF 10-32G, Ø 1,6 mm , PEEK","10 x","1 db","F 830-10; BOLA"]
[9,"Tubing Cutter, a Ø 28 mm, STEEL","1 x","1 db","S 1852-28; BOLA"]
[10,"Heat-Shrinkable Tubing, max. iØ 1,98 mm-> min. 0,7 , PTFE","3 x","1 m","S 1828-08 (3 m); BOLA"]
[11,"Heat-Shrinkable Tubing, max. iØ 3,2 mm-> min. 1,0 , PTFE","3 x","1 m","S 1828-16 (3 m); BOLA"]
[12,"Temperature Probes (PT 100), Ø 8 mm, L 660 mm, PTFE/PFA","2 x","1 db","P 1750-30; BOLA"]
[13,"Miniature 3-Way Stopcocks, UNF 1/4\" 28G, Ø 0,8 x 1,6 , PTFE","1 x","1 db","F 731-02; BOLA"]
[]
[]
[]
["Ssz.","Megnevezés","Mennyiség","Kiszerelés","Kompatibilitás"]
[1,"VALVE, MANUAL, 4-PORT, HIGH PRESSURE","2 x","1 db","001122; Omnifit"]