{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Munka1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Munka1","index":0,"n_rows":21,"n_cols":3,"rows_kept":21,"cut":false,"hidden":false,"merged":[]}
["SZTE FOK „A” épület kompresszor helyiségek elektromos hálózatának kiépítése"]
[]
[]
[]
["Bontási munkák","Anyag","Díj"]
["Kábelek bontása"]
["Elosztó szekrény bontása"]
[]
["Szerelési munkák"]
["Betáp kábel meglévő védőcsőbe húzása NYYJ-5×35mm2        10m"]
["Fő-elosztó szerelése és bekötése"]
["Gépészeti szakasz-elosztó elkészítése,bekötése"]
["Gépészeti al-elosztó elkészítése,bekötése"]
["Csatlakozás kiépítése 32A-ig  (10m-ig)   3db"]
["Átadási dokumentáció elkészítése (műszaki leírás szerint)"]
[]
["Összesen"]
[]
["Mindösszesen (nettó)",{"$f":"SUM(B6:B15)","v":0},{"$f":"SUM(C6:C15)","v":0}]
["ÁFA (%)",0.27,0.27]
["Bruttó",{"$f":"(B19*1.27)","v":0},{"$f":"(C19*1.27)","v":0}]