{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["építészet"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"építészet","index":0,"n_rows":18,"n_cols":8,"rows_kept":18,"cut":false,"hidden":false,"merged":[[3,2,3,3],[13,6,13,7],[15,6,15,7],[17,6,17,7],[2,4,2,5]],"flags":["formulas_cached_only"]}
[null,"SZTE MK Élelmiszermérnöki Intézet – Érzékszervi laboratórium eszközeinek beépítése"]
[null,"Villanyszerelés"]
[{"$nulls":4},"Egységár"]
[null,"Tétel","Mennyiség",null,"anyag díj","munkadí díj","Anyag összesen","díj összesen"]
[]
[]
[]
["1.","Mosogatógép dugalj áramkör kiépítése főelosztóból C16A (1ÁK) IP44 fk.dugaljal",1,"klt",0,0,0,0]
["2.","Műanyag vezeték csatornába építhető dugalj (IP55) bekötev,kábelezve,meglévő áramkör felhasználásával",1,"klt",0,0,0,0]
["3.","EPH hálózat kialakítása főelosztóból",1,"klt",0,0,0,0]
["4.","Érintésvédelmi mérés és jegyzőkönyv készítése",1,"klt",0,0,0,0]
[null,"Anyag összesen",{"$nulls":4},0]
[null,"Munkadíj összesen",{"$nulls":5},0]
[null,"Nettó összesen",{"$nulls":4},0]
[]
[null,"ÁFA 27 %",{"$nulls":4},0]
[]
[null,"ÖSSZESSEN Bruttó",{"$nulls":4},0]