{"text_format":"2","workbook":"xlsx","n_sheets":2,"sheets":["Sheet2","Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet2","index":0,"n_rows":10,"n_cols":3,"rows_kept":10,"cut":false,"hidden":false,"merged":[]}
["Termékkód","Igényelt mennyiség","Megnevezés"]
["05.001.601",1,"UNIUM MODULAR DRIVE HANDPIECE"]
["05.001.602",1,"UNIUM POWER UNIT"]
["05.001.603",1,"UNIUM STERILE COVER"]
["05.001.604",1,"UNIUM ADAPTER F/UBC II"]
["05.001.250",1,"AO/ASIF gyorscsatoló 532.001"]
["05.001.188",1,"QC Ø0.6-3.2 F/UNIUM"]
["532.021",1,"Oszcillációsfűrész-feltét"]
["532.011",1,"Mini gyorscsatoló 532.001"]
["05.001.252",1,"Fúrófeltét fúrási sebesség"]

{"sheet":"Sheet1","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}