{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["Munka1","Munka2","Munka3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Munka1","index":0,"n_rows":13,"n_cols":21,"rows_kept":13,"cut":false,"hidden":false,"merged":[[7,20,12,20],[11,10,11,11],[11,13,11,14],[12,2,12,3],[12,4,12,5],[12,6,12,7],[12,8,12,9],[12,10,12,11],[12,13,12,14],[12,16,12,17],[7,16,7,17],[8,16,8,17],[9,16,9,17],[10,16,10,17],[11,16,11,17],[7,19,11,19],[7,10,7,12],[8,10,8,12],[9,10,9,12],[10,10,10,12],[7,13,7,15],[8,13,8,15],[9,13,9,15],[10,13,10,15],[8,6,8,7],[9,6,9,7],[10,6,10,7],[11,6,11,7],[7,8,7,9],[8,8,8,9],[9,8,9,9],[10,8,10,9],[11,8,11,9],[6,17,6,18],[7,0,12,0],[7,1,11,1],[7,2,7,3],[8,2,8,3],[9,2,9,3],[10,2,10,3],[11,2,11,3],[7,4,11,5],[7,6,7,7],[4,11,5,13],[4,14,5,16],[4,17,5,18],[6,1,6,2],[6,3,6,4],[6,5,6,6],[6,7,6,8],[6,9,6,10],[6,11,6,13],[6,14,6,16],[2,14,2,18],[3,14,3,18],[1,19,5,19],[1,20,6,20],[4,1,5,2],[4,3,4,4],[5,3,5,4],[4,5,5,6],[4,7,5,8],[4,9,5,10],[0,1,0,19],[1,0,6,0],[1,1,3,4],[1,5,1,8],[2,5,2,8],[3,5,3,8],[1,9,1,13],[2,9,2,13],[3,9,3,13],[1,14,1,18]]}
["Product","Specification",{"$nulls":18},"Quantity"]
["X-Ray Photodiode ","Active area",null,null,null,"Capacitance",null,null,null,"Shunt resistance",{"$nulls":4},"NEP",{"$nulls":4},"Package style",1]
[{"$nulls":5},"(nF)",null,null,null,"(MΩ)",{"$nulls":4},"(W/√Hz)"]
[{"$nulls":5},"0V",null,null,null,"-10 mV"]
[null,"Area (mm²)",null,"Dimensions",null,"typ.",null,"max.",null,"min.",null,"typ.",null,null,"typ.",null,null,"max."]
[null,null,null,"(mm)"]
[null,100,null,"10,00 sq",null,6,null,8,null,10,null,100,null,null,1.3E-14,null,null,4.1000000000000002E-14,null,"25/ceramic"]
["Photodiode ","Area (mm²)","Dimensions",null,"Peak responsivity Wavelength (nm)",null,"Responsivity (A/W)",null,"Depletion Voltage",null,"Dark Current (nA)",null,null,"Capacitance (pF)",null,null,"NEP",null,"Reverse Voltage (V)","Package style",2]
[null,null,"(mm)",null,null,null,"900 nm",null,"V",null,"-100 V",null,null,"-100 V",null,null,"(W/√Hz)",null,"10μA"]
[{"$nulls":6},"typ.",null,"typ",{"$nulls":7},"900nm",null,"max."]
[{"$nulls":16},"-100V"]
[{"$nulls":10},"typ.",null,"max.","typ.",null,"max.","typ."]
[null,100,"10 Sq",null,950,null,0.6,null,75,null,"2†",null,"10†","50†",null,"60†","3,2 e-14",null,120,"25/ceramic"]

{"sheet":"Munka2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Munka3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}