{"text_format":"2","workbook":"xls","n_sheets":2,"sheets":["KSZF","Munka3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"KSZF","index":0,"n_rows":12,"n_cols":7,"rows_kept":12,"cut":false,"hidden":false,"merged":[[11,0,11,5]],"flags":["formulas_cached_only"]}
["Termék / szolgáltatás megnevezése"," szállítási egység","Mértékegység","Szerződéses ár (nettó) (Ft)","Jótállási idő\n(hónap)","Ár (bruttó + kbdíj)","Összesen  (Ft)"]
["19” 1U Patch Panel, 16 x RJ45/s, Cat.6",1,"db",null,"60",0,0]
["19“ csatornás patch rendező 1U",1,"db",null,12,0,0]
["Real10 S/FTP 4P 650 MHz     LSOH",180,"m",null,120,0,0]
["Falikábel behúzás",180,"m",null,12,0,0]
["Végpont szerelés",18,"db",null,"12",0,0]
["Connection Module Cat.6 100xRJ45/s",9,"db",null,60,0,0]
["Fali süllyesztett aljzatt, 88x88, 2x1Port, fehér",5,"db",null,60,0,0]
["Falon kívüli Csatorna szerelése",16,"m",null,"12",0,0]
["Műanyag fali kábelcsatorna fedéllel 040*060",14,"m",null,12,0,0]
["Műanyag fali kábelcsatorna fedéllel 060*130",2,"m",null,12,0,0]
["Szumma",{"$nulls":5},0]

{"sheet":"Munka3","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}