{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Munka1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Munka1","index":0,"n_rows":30,"n_cols":2,"rows_kept":30,"cut":false,"hidden":false,"merged":[[0,0,0,1],[70,0,70,1],[57,0,57,1],[1,0,1,1],[11,0,11,1],[19,0,19,1],[31,0,31,1],[43,0,43,1]]}
["JUGYU BÁL 2023"]
[]
["Hangtechnika","Mennyiség"]
["Sub hangsugárzó (min.140dB, 2x18\")",2]
["Basszus hangsugárzó (min.140dB, 1x15\")",2]
["Közép-magas hangsugárzó (min. 145dB, 2x10\", 1x3\")",2]
["Sub hangsugárzó (min.140dB, 1x18\")",1]
["Monitor hangsugárzó (min. 136dB, 1x15\", 1x3\")",4]
["Vezetéknélküli mikrofon (Shure, Sennheiser)",2]
["Digitális keverőpult (min. 32csatorna, Yamaha,Avid,Digico)",1]
[]
["Fénytechnika"]
["Wash robotlámpa (min. 19x15W LED v. ezzel megegyező)",12]
["Spot robotlámpa (min. 120W LED v. ezzel megegyező)",2]
["Beam robotlámpa (min. 130W)",4]
["RGB Par lámpa (min. 120W LED v. Ezzel megegyezző, IP65)",18]
["Profil lámpa (min. 650W)",8]
["Fényvezérlő (min. 2univerzum)",1]
[]
["Színpadtechnika"]
["6x4m színpad 60cm magasan",1]
["2x2m dobdobogó",1]
["7x5m keret",1]
[]
["Személyzet"]
["Fénytechnikus",1]
["Hangtechnikus",2]
[]
["Szállítás, Építés, Bontás",1]
["Kordon","25m"]