{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Munka1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Munka1","index":0,"n_rows":12,"n_cols":1,"rows_kept":12,"cut":false,"hidden":false,"merged":[[2,0,3,0]]}
["MŰSZAKI LEÍRÁS"]
["Vibrációs golyósmalom kis mennyiségű minták nagy finomságú őrlésére és porok keverésére, 1 db"]
["Minimum paraméterek"]
[]
["Munkahelyek száma 2 db"]
["Digitális idő és frekvencia kijelzés: legalább 3 program tárolására alkalmas"]
["Rázatási frekvencia 3-25 Hz (180-1500 ford./perc)"]
["Bemenő szemcseméret < 6 mm"]
["Kimenő szemcseméret <10"]
["Minta térfogata max. 2*10 ml"]
["Teljesítmény legalább 100 Watt"]
["Kompatibilis a 10 ml-es MM 200 golyósmalomba való wolfram-karbid őrlőedényekkel"]