{"text_format":"2","workbook":"xlsx","n_sheets":2,"sheets":["I. részajánlati kör","II. részajánlati kör"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"I. részajánlati kör","index":0,"n_rows":82,"n_cols":11,"rows_kept":82,"cut":false,"hidden":false,"merged":[[0,0,0,10],[77,0,77,7],[80,0,80,10],[81,0,81,10],[79,0,79,10]]}
["I. részajánlati kör"]
["Sor","Megnevezés","minőség","m3/kg","űrtartalom"," db","Nettó egységár (Ft)","Bruttó egységár (Ft)","Nettó ár összesen (Ft)","Bruttó ár összesen (Ft)","Nyomás (bar)"]
["1.","Szintetikus levegő HC Free","5.0","10 m3","50 L","7",{"$nulls":4},200]
["2.","Szintetikus levegő","ipari","6 m3","40 L","54",{"$nulls":4},150]
["3.","Szintetikus levegő","ipari","1,5 m3","14 L","2",{"$nulls":4},150]
["4.","Szén-dioxid","élelmiszerip.","10 kg","14 L","24"]
["5.","Szén-dioxid","élelmiszerip.","20 kg","27 L","41"]
["6.","Szén-dioxid","élelmiszerip.","30 kg","40 L","41"]
["7.","Szén-dioxid","4.5","10 kg","14 L","2"]
["8.","Szén-dioxid (CO2) ","4.8 ","1,5 m3","10 L",1,{"$nulls":4},150]
["9.","Szén-dioxid (CO2)","4.8","7,5 m3","50 L",1,{"$nulls":4},150]
["10.","Szén-monoxid (CO) ","4.7  (100%)","1,5 m3","10 L",1,{"$nulls":4},150]
["11.","Szén-monoxid (CO) ","4.7  (100%)","7,5 m3","50 L",1,{"$nulls":4},150]
["12.","Oxigén (O2)","2.5 (100%)","1,5 m3","10 L",1,{"$nulls":4},150]
["13.","Oxigén (O2)","2.5 (100%)","7,5 m3","50 L",1,{"$nulls":4},150]
["14.","Oxigén","ipari","1,5 m3","10 L","5",{"$nulls":4},150]
["15.","Oxigén","ipari","6 m 3","40 L","29",{"$nulls":4},150]
["16.","Nitrogén","5.0","1.5m 3","10L","4",{"$nulls":4},150]
["17.","Nitrogén","5.0","6 m 3","40 L","34",{"$nulls":4},150]
["18.","Nitrogén","5.0","10 m3","50 L","23",{"$nulls":4},200]
["19.","Nitrogén","4.5","6 m 3","40 L","75",{"$nulls":4},150]
["20.","Nitrogén","4.5","2 m 3","10 L","1",{"$nulls":4},200]
["21.","Nitrogén","4.5","1.5m 3","10 L","1",{"$nulls":4},150]
["22.","Nitrogén","4.5","10 m3","50 L","163",{"$nulls":4},200]
["23.","Hidrogén","ipari","6 m3","40 L","2",{"$nulls":4},150]
["24.","Hidrogén","ipari","1,75 m3","14 L","1",{"$nulls":4},125]
["25.","Hidrogén","5.0","10 m 3","50 L","10",{"$nulls":4},200]
["26.","Hidrogén","5.0","1.5 m3","10 L","1",{"$nulls":4},150]
["27.","Hélium","4.6","1,5 m3","10 L","1",{"$nulls":4},150]
["28.","Hélium","4.6","2 m3","14 L","1",{"$nulls":4},200]
["29.","Hélium","4.6","6 m3","40 L","3",{"$nulls":4},150]
["30.","Hélium","4.6","10 m3","50 L","20",{"$nulls":4},200]
["31.","Hélium","5.0","2 m3","14 L","1",{"$nulls":4},200]
["32.","Hélium","5.0","10 m3","50 L","9",{"$nulls":4},200]
["33.","Hélium","6.0","10 m3","50 L","16",{"$nulls":4},200]
["34.","Argon","4.6","6 m3","40 L","7",{"$nulls":4},150]
["35.","Argon","4.6","10 m3","50 L","53",{"$nulls":4},200]
["36.","Argon","5.0","6 m3","40 L","14",{"$nulls":4},150]
["37.","Argon","5.0","1,5 m3","10L","3",{"$nulls":4},150]
["38.","Argon","5.0","10,7 m3","50L","3",{"$nulls":4},"200"]
["39.","Disszugáz","ipari","2 kg","14 L","1"]
["40.","Disszugáz","ipari","4 kg","27 L","1"]
["41.","Disszugáz","ipari","6 kg","40 L","1"]
["42.","Disszugáz","2.6","6 kg","40 L","2"]
["43.","Carbogén","CO2 O2-ben","6 m3","40 L","53",{"$nulls":4},150]
["44.","Carbogén","CO2 O2-ben","2 m3","10 L","13",{"$nulls":4},150]
["45.","Carbogén","CO2 N2-ben","6 m3","40 L","1",{"$nulls":4},150]
["46.","Carbogén","CO2 N2-ben","1,5 m3","10 L","1",{"$nulls":4},150]
["47.","Szárazjég  3mm, 16 mm",null,"kg",null,"36"]
["48.","Szárazjég tömb ",null,"kg",null,"8"]
["49.","Gázkeverék C18",null,"7 m3","40 L","1",{"$nulls":4},150]
["50.","Ammónia","ipari","20 kg","40 L","1"]
["51.","Kén-hidrogén","ipari","6,7 kg","10 L","1"]
["52.","Metán","4.5","12 m3","50 L","1",{"$nulls":4},200]
["53.","Metán","4.5","2,5 m3","10 L","1",{"$nulls":4},200]
["54.","Metán","2.5","12 m3","50 L","1",{"$nulls":4},200]
["55.","Metán","3.5","2 m3","10 L","1",{"$nulls":4},200]
["56.","Metán","3.5","12 m3","50 L","1",{"$nulls":4},200]
["57.","Szén-dioxid","5.5","37,5 kg","50 L","1"]
["58."," Kén-hidrogén nitrogénben","200ppm","1,5 m3","10 L","1",{"$nulls":4},150]
["59.","Kén-hidrogén metánban","200ppm","1,5 m3","10 L","1",{"$nulls":4},150]
["60.","Ammónia nitrogénben","5ppm","6 m3","40 L","1",{"$nulls":4},150]
["61.","Szén-dioxid nitrogénben","1%","6 m3","40 L","1",{"$nulls":4},150]
["62.","Metán nitrogénben","1%","6 m3","40 L","1",{"$nulls":4},150]
["63.","BTX nitrogénben","1ppm","1,5 m3","10 L","1",{"$nulls":4},150]
["64.","Fluor héliumban","5%","1,6 m3","10 L","1",{"$nulls":4},150]
["65."," Kén-hidrogén N2-ben","2%","6 m3","50 L","1",{"$nulls":4},150]
["66."," Kén-hidrogén N2-ben","2000ppm","6 m3","50 L","1",{"$nulls":4},150]
["67."," Kén-hidrogén N2-ben","200ppm","6 m3","50 L","1",{"$nulls":4},150]
["68."," Metán 4.5 Hélium 5.0-ban","5%","5 m3","40 L","1",{"$nulls":4},150]
["69.","Metán 4.5  Hélium 5.0-ban","5%","1.5 m3","10 L","1",{"$nulls":4},150]
["70.","Oxigén 4.5  Hélium 5.0-ban","10%","5 m3","40 L","1",{"$nulls":4},150]
["71.","Oxigén 5.0 10% Hélium 5.0-ban","10%","1,5 m3","10 L","1",{"$nulls":4},150]
["72.","Palack reduktor ipari 200/10 bar","4.8 -ig",null,null,"8"]
["73.","Palack reduktor labor 200/10 bar","6.0 -ig",null,null,"4"]
["74.","Cseppfolyós Hélium NMR befejtéssel","4.6","1 liter",null,"23"]
["75.","Reduktor tömítés",null,null,null,"2"]
["Végösszeg:",{"$nulls":7},{"$f":"SUM(I3:I77)","v":0},{"$f":"SUM(J3:J77)","v":0}]
[]
["Szállítási határidő:"]
["1-49. sorok esetében: megrendeléstől számított 72 órán belül"]
["50-75. sorok esetében: megrendeléstől számított maximum 12 héten belül"]

{"sheet":"II. részajánlati kör","index":1,"n_rows":2,"n_cols":11,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
["Sor","Megnevezés","minőség","m3/kg","űrtartalom","L","Nettó egységár (Ft)","Bruttó egységár (Ft)","Nettó ár összesen (Ft)","Bruttó ár összesen (Ft)","Nyomás (bar)"]
["76.","Cseppfolyós Nitrogén dewar edénybe fejtéssel","2.5","1 liter",null,15000]