{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Munka1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Munka1","index":0,"n_rows":44,"n_cols":6,"rows_kept":44,"cut":false,"hidden":false,"merged":[[1,0,3,0],[4,0,28,0],[29,0,43,0]]}
["Részajánlati körök","#","Eszköz","Gyártó","Típus","Mennyiség (db)"]
[1,1,"Flexibilis cső a cella csatlakozáshoz","Swagelok / S-Lok","SS-FM16SL16SL16-24 / SHFH16-S16-24-S6",2]
[null,2,"Flexibilis tömlő ","Swagelok / S-Lok","SS-FL8SL8SL8-200CM / SFH8-S8-2000L-S6",4]
[null,3,"Flexibilis tömlő ","Swagelok / S-Lok","SS-FL8sl8SL8-150CM / SFH8-S8-1500L-S6",1]
[2,4,"Biztonsági szelep","Swagelok / S-Lok","SS-R4S8 / SRV60-S-8T-S6",1]
[null,5,"Tűszelep, regulating stem","Swagelok / S-Lok","SS-1RS4 / SNV2-S-4T-R-S6",1]
[null,6,"Tűszelep, PCTFE stem","Swagelok / S-Lok","SS-1KS4 / SNV2-S-4T-K-S6",1]
[null,7,"1/4 tube fitting check valve","Swagelok / S-Lok","SS-CHS4-1 / SCH1-S-4T-1-S6",3]
[null,8,"Cső fitting, union könyök","Swagelok / S-Lok","SS-400-9 / SL-4-S6",21]
[null,9,"Cső fitting, 1/4 union T tube fitting","Swagelok / S-Lok","SS-400-3 / ST-4-S6",12]
[null,10,"Cső fitting G1/4 menettel - 1/4 tube fitting","Swagelok / S-Lok","SS-400-1-4RP / SOM-4-4G-S6",6]
[null,11,"1/4 cső fitting 1/4 NPT","Swagelok / S-Lok","SS-400-1-4 / SMC-4-4N-S6",4]
[null,12,"Cső fitting, 1/4 FEMALE NPT - 1/4 tube fitting","Swagelok / S-Lok","SS-400-7-8RG / SCG-4-8G-S6",5]
[null,13,"Cső fitting 1/4 union falátmenet","Swagelok / S-Lok","SS-400-61 / SUB-4-S6",3]
[null,14,"Cső fitting, 1/4 adapter - 1/4 male NPT","Swagelok / S-Lok","SS-4-TA-1-4 / SAM-4-4N-S6",12]
[null,15,"Stainless steel 1/8 union T tube fitting","Swagelok / S-Lok","SS-200-3 / ST-2-S6",8]
[null,16,"Stainless Steel Poppet Check Valve, Fixed Pressure, 1/8 in. Swagelok Tube Fitting, 1/3 psig (0.03 bar)","Swagelok / S-Lok","SS-2C-1/3 / SCV1-S-2T-1/3-S6",4]
[null,17,"Stainless Steel 1-Piece 40GGG Series 3-Way Ball Valve, 0.90 Cv, 1/8 in. Swagelok Tube Fitting","Swagelok / S-Lok","SS-41GXS2 / SBV1G-3B-S-2T-S6",1]
[null,18,"Stainless Steel 1/8 tube fitting - G1/8","Swagelok / S-Lok","SS-200-1-2RT / SMC-2-2R-S6",10]
[null,19,"Nagynyomású golyóscsap","Swagelok / S-Lok","SS-8GBF8 + 2 db SS-400-1-8 / SFBV2-S-4T-S6",2]
[null,20,"Visszacsapó szelepek gázkezelésekhez","Swagelok / S-Lok","SS-CHS4-5 / SCH1-S-4T-5-S6",7]
[null,21,"Manuális útváltó szelep","Swagelok / S-Lok","SS-43GXS4 / SBV2G-3B-S-4T-S6",2]
[null,22,"Biztonsági szelep CO2 katódoldal","Swagelok / S-Lok","SS-RL3M4F4-RT-SET_11barg-EP / SRV30-MF-4R-L11B-EP-S6",1]
[null,23,"Biztonsági szelep CO2 anódoldal","Swagelok / S-Lok","SS-RL3S4-SET_9barg-EP / SRV30-S-4T-L-9B-S6",1]
[null,24,"Biztonsági szelep H2 anódoldal","Swagelok / S-Lok","SS-RL3M4F4-RT-SET_9barg-EP / SRV30-MF-4R-L9B-S6",1]
[null,25,"Szűrő anolithoz","Swagelok / S-Lok","SS-8TF-15 / SFT3-S-8T-15-S6",2]
[null,26,"Tartalék szűrőbetét anolithoz","Swagelok / S-Lok","SS-8F-K4-15 / XEM-C-15-S6",2]
[null,27,"Szűrő katód gázhoz","Swagelok / S-Lok","SS-4TF-2 / SFT1-S-4T-2-S6",1]
[null,28,"Tartalék szűrőbetét katód gázhoz","Swagelok / S-Lok","SS-4F-K4-2 / XEM-A-2-S6",1]
[3,29,"1/4 tube fitting check valve","Swagelok","6L-CW4S4",5]
[null,30,"Stainless steel tubing 1/4_0,028 in thickness (2 m-es szálak)","Swagelok / S-Lok","SS-T4-S-035-6ME / 6,35x0,89 1.4404",30]
[null,31,"PFA cső, 1/8\" OD","Swagelok","PFA-T2-030-100 (100 feet ~ 30,48 m)",1]
[null,32,"FX 1/4 flexicső 1/4 tube fitting csatlakozásokkal","Swagelok","SS-FX 4 SL4 SL4 40CM-H7",1]
[null,33,"FX 1/4 flexicső 1/4 tube fitting csatlakozásokkal","Swagelok","SS-FX 4 SL4 SL4 45CM-H7",1]
[null,34,"FX 1/4 flexicső 1/4 tube fitting csatlakozásokkal","Swagelok","SS-FX 4 SL4 SL4 65CM-H7",1]
[null,35,"FX 1/4 flexicső 1/4 tube fitting csatlakozásokkal","Swagelok","SS-FX 4 SL4 SL4 60CM-H7",1]
[null,36,"FX 1/4 flexicső 1/4 tube fitting és male NPT csatival","Swagelok","SS-FX 4 SL4 PM4 80CM-H7",1]
[null,37,"FX 1/4 flexicső 1/4 male NPT mindkét oldalt 3méter","Swagelok","SS-FX 4 PM4 PM4 300CM-H7",1]
[null,38,"PTFE 1/8 tube fitting - G1/8","Swagelok","T-200-1-2RS",4]
[null,39,"PTFE T-elem 1/8\" tube fitting ","Swagelok","T-200-3",2]
[null,40,"PTFE 1/8 tube fitting - 1/4 NPT ","Swagelok","T-2-TA-7-4",1]
[null,41,"Tömítőkészlet biztonsági szelepbe","Swagelok / S-Lok","EP-R3A-K2 / SRV60-SKIT",3]
[null,42,"Flow limiter nitrogén öblítéshez","Swagelok / S-Lok","SS-200-6 PD LD-.0079 / SU-2-PD-OF2-S6",2]
[null,43,"Flow limiter H2 katód nyomásmentesítéséhez","Swagelok","SS-400-6 PD LD-.001",1]