{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Specification"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Specification","index":0,"n_rows":202,"n_cols":10,"rows_kept":202,"cut":false,"hidden":false,"merged":[]}
[null,null,null,"Specification for Call for Proposals No SZTE/2024/PB13771"]
["Part","#","Description","Connection 1","Connection 2","Tube diameter","Design pressure","Reference Swagelok/Schwer factory code","Quantity","Comment"]
["I.",1,"One piece ball valve","1/2\" G","-","-","-","A-BV1XG12-8i",12]
["I.",2,"One piece ball valve","1/4\" G","-","-","-","A-BV1XG14-8i",2]
["I.",3,"One piece ball valve","1\" G","-","-","-","A-BV1XG1-8i",3]
["I.",4,"One piece ball valve","3/4\" G","-","-","-","A-BV1XG34-8i",6]
["I.",5,"One piece ball valve","1/2\" NPT","-","-","-","A-BVEN12-8i",1]
["I.",6,"Check valve","1/4\" G","-","-","-","A-CV1G114-2E",1]
["I.",7,"3-piece ball valve","D 15 tube","D 15 tube","-","-","A-KH15-5i PTFE",6]
["I.",8,"3-piece ball valve","D 28 tube","D 28 tube","-","-","A-KH28-5i PTFE",1]
["I.",9,"3-piece ball valve","D 54 tube","D 54 tube","-","-","A-KH54-5i PTFE",2]
[null,null,"PLUS SHIPPING COST"]
[]
["II.",10,"45° Elbow","D 15 tube","D 15 tube","-","-","Aq-45B15-4LVm",22]
["II.",11,"45° Elbow","D 15 tube","1/2\" R","-","-","Aq-45B15R12-4LVm",1]
["II.",12,"45° Elbow","D 22 tube","D 22 tube","-","-","Aq-45B22-4LVm",5]
["II.",13,"45° Elbow","D 28 tube","D 28 tube","-","-","Aq-45B28-4LVm",6]
["II.",14,"45° Elbow","D 54 tube","D 54 tube","-","-","Aq-45B54-4LVm",2]
["II.",15,"90° Elbow","D 15 tube","-","-","-","Aq-90Bia15-4LVm",32]
["II.",16,"90° Elbow","D 18 tube","-","-","-","Aq-90Bia18-4LVm",2]
["II.",17,"90° Elbow","D 22 tube","-","-","-","Aq-90Bia22-4LVm",2]
["II.",18,"90° Elbow","D 28 tube","-","-","-","Aq-90Bia28-4LVm",10]
["II.",19,"90° Elbow","D 42 tube","-","-","-","Aq-90Bia42-4LVm",1]
["II.",20,"90° Elbow","D 54 tube","-","-","-","Aq-90Bia54-4LVm",7]
["II.",21,"Valve Connector","D 15 tube","1 1/4\" G","-","-","Aq-AV15G114VA-4LVm",2]
["II.",22,"Valve Connector","D 15 tube","3/4\" G","-","-","Aq-AV15G34VA-4LVm",75]
["II.",23,"Valve Connector","D 18 tube","3/4\" G","-","-","Aq-AV18G34VA-4LVm",6]
["II.",24,"Valve Connector","D 22 tube","1\" G","-","-","Aq-AV22G1VA-4LVm",17]
["II.",25,"Valve Connector","D 28 tube","1 1/4\" G","-","-","Aq-AV28G114VA-4LVm",17]
["II.",26,"Valve Connector","D 35 tube","1 1/2\" G","-","-","Aq-AV35G112VA-4LVm",2]
["II.",27,"Valve Connector","D 54 tube","2 3/8\" G","-","-","Aq-AV54G238VA-4LVm",2]
["II.",28,"90° Elbow","D 15 tube","D 15 tube","-","-","Aq-B15-4LVm",95]
["II.",29,"90° Elbow","D 15 tube","1/2\" R","-","-","Aq-B15R12-4LVm",1]
["II.",30,"90° Elbow","D 18 tube","D 18 tube","-","-","Aq-B18-4LVm",3]
["II.",31,"90° Elbow","D 22 tube","D 22 tube","-","-","Aq-B22-4LVm",12]
["II.",32,"90° Elbow","D 28 tube","D 28 tube","-","-","Aq-B28-4LVm",9]
["II.",33,"90° Elbow","D 42 tube","D 42 tube","-","-","Aq-B42-4LVm",1]
["II.",34,"90° Elbow","D 54 tube","D 54 tube","-","-","Aq-B54-4LVm",14]
["II.",35,"Straight Coupling","D 22 tube","D 22 tube","-","-","Aq-M22-4LVm",1]
["II.",36,"Straight Coupling","D 42 tube","D 42 tube","-","-","Aq-M42-4LVm",1]
["II.",37,"Straight Coupling","D 54 tube","D 54 tube","-","-","Aq-M54-4LVm",5]
["II.",38,"MF Reducer","D 22 tube","D 15 tube","-","-","Aq-RS2215-4LVm",{"$f":"4+1","v":5}]
["II.",39,"MF Reducer","D 42 tube","D 15 tube","-","-","Aq-RS4215-4LVm",{"$f":"2+4","v":6}]
["II.",40,"MF Reducer","D 42 tube","D 28 tube","-","-","Aq-RS4228-4LVm",3]
["II.",41,"MF Reducer","D 54 tube","D 18 tube","-","-","Aq-RS5418-4LV",1]
["II.",42,"MF Reducer","D 54 tube","D 22 tube","-","-","Aq-RS5422-4LV",{"$f":"3+1","v":4}]
["II.",43,"MF Reducer","D 54 tube","D 28 tube","-","-","Aq-RS5428-4LV",10]
["II.",44,"MF Reducer","D 54 tube","D 35 tube","-","-","Aq-RS5435-4LV",2]
["II.",45,"MF Reducer","D 54 tube","D 42 tube","-","-","Aq-RS5442-4LV",2]
["II.",46,"Tee","D 15 tube","D 15 tube","D 15","-","Aq-T15-4LVm",19]
["II.",47,"Tee","D 22 tube","D 22 tube","D 22","-","Aq-T22-4LVm",5]
["II.",48,"Tee","D 28 tube","D 28 tube","D 28","-","Aq-T28-4LVm",2]
["II.",49,"Tee","D 42 tube","D 42 tube","D 42","-","Aq-T42-4LVm",3]
["II.",50,"Tee","D 54 tube","D 54 tube","D 54","-","Aq-T54-4LVm",5]
["II.",51,"Tee","D 22 tube","D 15 tube","D 22","-","Aq-TA2215-4LVm",1]
["II.",52,"Tee","D 22 tube","1/2\" Rp","D 22","-","Aq-TA22Rp12-4LVm",3]
["II.",53,"Tee","D 28 tube","D 15 tube","D 28","-","Aq-TA2815-4LVm",3]
["II.",54,"Tee","D 28 tube","D 18 tube","D 28","-","Aq-TA2818-4LVm",1]
["II.",55,"Tee","D 54 tube","D 28 tube","D 54","-","Aq-TA5428-4LVm",8]
["II.",56,"Tee","D 54 tube","D 42 tube","D 54","-","Aq-TA5442-4LVm",{"$f":"1+4","v":5}]
["II.",57,"Tee","D 54 tube","2\" Rp","D 54","-","Aq-TA54Rp2-4LVm",2]
["II.",58,"Threaded Flange","DN 15","1/2\" Rp","-","-","F-GF15-16-40-3i",4]
["II.",59,"Male Adapter","D 15 tube","1/2\" R","-","-","Aq-US15R12-4LVm",4]
["II.",60,"Adapter Flange","D 22 tube","-","-","-","Aq-UF22-4LVm",{"$f":"1+1+1","v":3},"A 105"]
["II.",61,"Adapter Flange","D 42 tube","-","-","-","Aq-UF42-4LVm",6,"A 150"]
["II.",62,"Adapter Flange","D 28 tube","-","-","-","Aq-UF28-4LVm",2,"A 115"]
["II.",63,"Female Adapter","D 18 tube","3/4\" Rp","-","-","Aq-UM18Rp34-4LVm",1]
["II.",64,"Female Adapter","D 22 tube","1\" Rp","-","-","Aq-UM22Rp1-4LVm",2]
["II.",65,"Female Adapter","D 28 tube","1\" Rp","-","-","Aq-UM28Rp1-4LVm",5]
["II.",66,"Female Adapter","D 54 tube","1 1/2\" Rp","-","-","Aq-UM54Rp112-4LVm",4]
["II.",67,"Valve Connector","D 15 tube","3/4\" G","-","-","Aq-V15VA-4LVm",1]
["II.",68,"Valve Connector","D 15 tube","1/2\" Rp","-","-","Aq-VI15Rp12VA-4LV",1]
["II.",69,"Valve Connector","D 54 tube","2\" Rp","-","-","Aq-VI54Rp2VA-4LV",1]
["II.",70,"Plug","D 42 tube","-","-","-","Aq-VS42-4LVm",1]
["II.",71,"Plug","D 54 tube","-","-","-","Aq-VS54-4LVm",1]
["II.",72,"Welded Stainless Steel Pipes","-","-","D 15","-","TAq-R15x1-4LE",66,"specified in meters"]
["II.",73,"Welded Stainless Steel Pipes","-","-","D 18","-","TAq-R18x1-4LE",6,"specified in meters"]
["II.",74,"Welded Stainless Steel Pipes","-","-","D 22","-","TAq-R22x12-4LE",12,"specified in meters"]
["II.",75,"Welded Stainless Steel Pipes","-","-","D 28","-","TAq-R28x12-4LE",12,"specified in meters"]
["II.",76,"Welded Stainless Steel Pipes","-","-","D 35","-","TAq-R35x15-4LE",6,"specified in meters"]
["II.",77,"Welded Stainless Steel Pipes","-","-","D 42","-","TAq-R42x15-4LE",6,"specified in meters"]
["II.",78,"Welded Stainless Steel Pipes","-","-","D 54","-","TAq-R54x15-4LE",12,"specified in meters"]
["II.",79,"O-Ring","D 54","-","-","-","Aq-OR-E54",170,"EPDM, 54 mm"]
["II.",80,"O-Ring","D 42","-","-","-","Aq-OR-E42",50,"EPDM, 42 mm"]
["II.",81,"O-Ring","D 35","-","-","-","Aq-OR-E35",10,"EPDM, 35 mm"]
["II.",82,"O-Ring","D 28","-","-","-","Aq-OR-E28",120,"EPDM, 28 mm"]
["II.",83,"O-Ring","D 22","-","-","-","Aq-OR-E22",100,"EPDM, 22 mm"]
["II.",84,"O-Ring","D 18","-","-","-","Aq-OR-E18",20,"EPDM, 18 mm"]
["II.",85,"O-Ring","D 15","-","-","-","Aq-OR-E15",400,"EPDM, 15 mm"]
[null,null,"PLUS SHIPPING COST"]
[]
["III.",86,"Female Adapter","D 15 tube","1/2\" Rp","-","-","Aq-UM15Rp12-4LVm",8]
[null,null,"PLUS SHIPPING COST"]
[]
["IV.",87,"Blanking Plug","3/4\" G","-","-","-","HA-694G34",4]
["IV.",88,"Female Male Adapter","1\" NPT","1\" R","-","-","IC-FMA-N1R1-4L",3]
["IV.",89,"Hexagon Adapter","1\" NPT","1\" G","-","-","IC-HA-G1N1-RS-4L",1]
["IV.",90,"Male Stud Coupling","4LL","1/8\" R","-","-","SR-5104LLR18c",4]
["IV.",91,"Hexagonal Reducing Bush","1/2\" Ga","1/8\" G","-","-","SR-5431218",2]
["IV.",92,"Non-return Valve","1 1/2\" G","-","-","-","V-CVG11202-E",1,"Opening Pressure: ca. 0.2 bar"]
["IV.",93,"Hose Tap","1/2\" G","-","-","-","A-DTG12-4L",1]
["IV.",94,"In Line Filter","1/4\" NPT","1/4\" NPT","-","-","HyF-LFN14-40µm-4LP",2,"40 um"]
[null,null,"PLUS SHIPPING COST"]
[]
["V.",95,"Hexagon Nipple","1/2\" G","-","-","-","SR-505G12",10]
["V.",96,"Male Connector","1\" tube fitting","1\" NPT","-","-","u2-MCz1N1-4L",3]
[null,null,"PLUS SHIPPING COST"]
[]
["VI.",97,"Return Check Valve","1/2\" G","-","-","-","A-YCVG12-8i",1,"Opening Pressure: ca. 0.1 bar"]
["VI.",98,"Flat seals for Flanges","DN 32","-","-","-","F-DF32-10-40-E",2,"EPDM"]
["VI.",99,"Flat seals for Flanges","DN 40","-","-","-","F-DF40-10-40-E",2,"EPDM"]
["VI.",100,"Threaded Flange","1 1/4\" NPT","-","-","-","F-GFA114-150-4Li",2]
["VI.",101,"Socket","1\" G","-","-","-","GF-101G1-7",2]
["VI.",102,"Hexagonal Socket","1/2\" G","-","-","-","GF-101HEXG12-7",2]
["VI.",103,"Hexagonal Socket","1/4\" G","-","-","-","GF-101HEXG14-7",2]
["VI.",104,"Reducing Nipple","1\" G","1/4\" G","-","-","GF-105G114-7",2]
["VI.",105,"Reducing Nipple","1/2\" G","1/4\" G","-","-","GF-105G1214-7",2]
["VI.",106,"Reducing Nipple","1/4\" G","1/8\" G","-","-","GF-105G1418-7",6]
["VI.",107,"Reducing Nipple","3/4\" G","1/2\" G","-","-","GF-105G3412-7",35]
["VI.",108,"Reducing Nipple","3/4\" G","1/4\" G","-","-","GF-105G3414-7",4]
["VI.",109,"Hexagonal Bush","1\" Ga","1/2\" Gi","-","-","GF-106G112-7",1]
["VI.",110,"Hexagonal Bush","1 1/4\" Ga","1/2\" Gi","-","-","GF-106G11412-7",2]
["VI.",111,"Hexagonal Bush","1/2\" Ga","1/4\" Gi","-","-","GF-106G1214-7",2]
["VI.",112,"Hexagonal Bush","3/4\" Ga","1/4\" Gi","-","-","GF-106G3414-7",7]
["VI.",113,"Hexagonal Bush","1 1/4\" Ga","1\" Gi","-","-","GF-106G1141-7",7]
["VI.",114,"Hexagonal Bush","3/4\" Ga","1/2\" Gi","-","-","GF-106G3412-7",5]
["VI.",115,"Male Stud Coupling","1 1/2\" G","1 1/2\" NPT","-","-","HA-614G112N112",2]
["VI.",116,"Male Stud Coupling","1 1/2\" G","1 1/2\" R","-","-","HA-614G112R112",4]
["VI.",117,"Male Stud Coupling","1 1/4\" G","1 1/4\" NPT","-","-","HA-614G114N114",2]
["VI.",118,"Male Stud Coupling","1/2\" G","1/2\" NPT","-","-","HA-614G12N12",1]
["VI.",119,"Male Stud Coupling","1/2\" G","1/2\" R","-","-","HA-614G12R12",3]
["VI.",120,"Male Stud Coupling","1/4\" G","1/2\" NPT","-","-","HA-614G14N12",3]
["VI.",121,"Male Stud Coupling","1/4\" G","1/4\" NPT","-","-","HA-614G14N14",2]
["VI.",122,"Male Stud Coupling","1\" G","1\" NPT","-","-","HA-614G1N1",1]
["VI.",123,"Male Stud Coupling","3/4\" G","1\" NPT","-","-","HA-614G34N1",1]
["VI.",124,"Male Stud Coupling","3/4\" G","1/2\" NPT","-","-","HA-614G34N12",18]
["VI.",125,"Blanking Plug","1/2\" G","-","-","-","HA-694G12",3]
["VI.",126,"Blanking Plug","1/4\" G","-","-","-","HA-694G14",1]
[null,null,"PLUS SHIPPING COST"]
[]
["VII.",127,"Female Male Adapter","1/2\" NPT","1/2\" R","-","-","IC-FMA-N12R12-4L",3]
["VII.",128,"Female Male Adapter","3/4\" NPT","3/4\" R","-","-","IC-FMA-N34R34-4L",1]
["VII.",129,"Flat seals for Flanges","DN 15","-","-","-","F-DF15-10-40-E",4,"EPDM, IBC DN15 PN16"]
["VII.",130,"Flat seals for Flanges","DN 40","-","-","-","F-DF40-10-40-E",2,"EPDM, IBC DN40 PN16"]
["VII.",131,"Flat seals for Flanges","DN 20","-","-","-","F-DF20-10-40-E",1,"EPDM, IBC DN20 PN16"]
["VII.",132,"Flat seals for Flanges","DN 25","-","-","-","F-DF25-10-40-E",2,"EPDM, IBC DN20 PN16"]
["VII.",133,"Check Valve","1\" tube fitting","1\" tube fitting","-","-","u2-CVz1ps1-4LV",1,"Opening Pressure: 1 psi/0.07 bar"]
["VII.",134,"Female Connector","1/2\" tube fitting","1/2\" G","-","-","u2-FCz12G12-4L",3]
["VII.",135,"Female Connector","1/2\" tube fitting","1/2\" G","-","-","u2-FCz12G12-GJ-4",2]
["VII.",136,"Male Connector","1/4\" tube fitting","1/4\" G","-","-","u2-MCz14G14-ESE-4L",1]
["VII.",137,"Male Connector","1/4\" tube fitting","1/4\" NPT","-","-","u2-MCz14N14-4L",1]
["VII.",138,"Blind Flange","DN 20","-","-","-","F-BF20-10-40-3i",1,"05/B DN20 PN16"]
["VII.",139,"Non-return Valve","1\" G","-","-","-","V-CVG102-E",1,"Opening Pressure: ca. 0.2 bar"]
["VII.",140,"Non-return Valve","1/2\" G","-","-","-","V-CVG1202-E",7,"Opening Pressure: ca. 0.2 bar"]
[null,null,"PLUS SHIPPING COST"]
[]
["VIII.",141,"Hexagon Nipple","1\" G","-","-","-","SR-505G1",6]
["VIII.",142,"Hexagon Nipple","1 1/4\" G","-","-","-","SR-505G114",2]
["VIII.",143,"Hexagon Nipple","3/4\" G","-","-","-","SR-505G34",6]
[null,null,"PLUS SHIPPING COST"]
[]
["IX.",144,"Connector","1\" M NPT","1\" tube fitting","-","PN63","SS-1610-1-16/u2-MCz1N1-4L",7]
["IX.",145,"Connector","1/2\" M G","1\" tube fitting","-","PN63","SS-1610-1-8RS",1]
["IX.",146,"Tee Tube Fitting","3/4\" F NPT","1\" tube fitting","1\"","PN63","SS-1610-3-12TTF",1]
["IX.",147,"Reducing Union Tee Tube Fitting","1/2\" tube fitting","1\" tube fitting","1\"","PN63","SS-1610-3-16-8/u2-RTz1z1z12-4L",8]
["IX.",148,"Adapter","1\" tube adapter","1\" M G","-","PN63","SS-16-TA-1-16RS",1]
["IX.",149,"Adapter","1\" tube adapter","1/2\" M NPT","-","PN63","SS-16-TA-1-8",4]
["IX.",150,"Connector","3/8\" M G","1/4\" tube fitting","-","PN63","SS-400-1-6RS",6]
["IX.",151,"Check Valve","1/4\" tube fitting","1/4\" tube fitting","-","-","SS-4C-10/u2-CVz14ps10-4LV",3,"Opening Pressure: 10 psi/0.7 bar"]
["IX.",152,"Male-Shaft Adaptor for Soft Seal","1/4\" tube adapter","1/4\" M G","-","-","SS-4-TA-1-4RS/u2-MAXz14G14-ESV-4L",2]
["IX.",153,"Female Adapter","1/4\" tube adapter","1/4\" F G","-","-","SS-4-TA-7-4RG",3]
["IX.",154,"Union Tee","1/2\" tube fitting","1/2\" tube fitting","1/2\"","-","SS-810-3/u2-Tz12-4L",3]
["IX.",155,"Reducing Union","1/2\" tube fitting","1/4\" tube fitting","-","-","SS-810-61-4",6]
["IX.",156,"Female Connector","1/2\" tube fitting","1/2\" F NPT","-","-","SS-810-7-8/u2-FCz12N12-4L",2]
["IX.",157,"Reducer","1/2\" tube fitting","1/4\" tube adapter","-","-","SS-810-R-4/u2-URSz12z14-4L",1]
["IX.",158,"Male Tube Adapter","1/2\" tube adapter","1/2\" M G","-","-","SS-8-TA-1-8RS",2]
["IX.",159,"Female Tube Adapter","1/2\" tube adapter","1/2\" F NPT","-","-","SS-8-TA-7-8/u2-FAXz12N12-4L",1]
["IX.",160,"Stainless steel seamless tube","-","-","OD 1/4\"","PN63","SS-T4-S-035-20",12,"specified in meters"]
[null,null,"PLUS SHIPPING COST"]
[]
["X.",161,"Connector","1\" M G","1\" tube fitting","-","PN63","SS-1610-1-16RS/u2-MCz1G1-CS-4L",6]
["X.",162,"Connector","1/2\" M NPT","1\" tube fitting","-","PN63","SS-1610-1-8/u2-MCz1N12-4i-8",1]
["X.",163,"Union Tee Tube Fitting","1\" tube fitting","1\" tube fitting","1\"","PN63","SS-1610-3/u2-Tz1-4L",10]
["X.",164,"Reducing Union Tube Fitting","1\" tube fitting","1/2\" tube fitting","-","PN63","SS-1610-6-8/u2-RUz1z12-4L",4]
["X.",165,"Union Elbow","1\" tube fitting","1\" tube fitting","-","PN63","SS-1610-9/u2-Ez1-4L",26]
["X.",166,"Connector","1\" M NPT","1/4\" F NPT","-","PN63","SS-16-RB-4/IC-RB-N1N14-4L",2]
["X.",167,"Male Connector for Metal Seal","1/2\" tube fitting","1/4\" M G","-","-","SS-810-1-4RS/u2-MCz12G14-CS-4L",4]
["X.",168,"Male Connector for Metal Seal","1/2\" tube fitting","1/2\" M G","-","-","SS-810-1-8RS/u2-MCz12G12-CS-4L",4]
["X.",169,"Male Connector","1/2\" tube fitting","1/8\" M NPT","-","-","SS-810-1-2",1]
["X.",170,"Male Connector","1/2\" tube fitting","1/2\" M NPT","-","-","SS-810-1-8",4]
["X.",171,"Union Elbow","1/2\" tube fitting","1/2\" tube fitting","-","-","SS-810-9/u2-Ez12-4Li",20]
["X.",172,"Adapter","1/2\" F NPT","1/2\" R","-","-","SS-8-A-8RT/IC-FMA-N12R12-4L",5]
["X.",173,"Check Valve","1/2\" tube fitting","1/2\" tube fitting","-","-","SS-8C-10",1]
["X.",174,"Female Tube Adapter","1/2\" tube adapter","1/2\" F G","-","-","SS-8-TA-7-8RG/u2-GFAXz12G12-4L",1]
[null,null,"PLUS SHIPPING COST"]
[]
["XI.",175,"Adapter Flange","DN 15","1/2\" tube fitting","-","PN16","SS-810-F15E-16-B1",2,"raised face, serrated"]
[null,null,"PLUS SHIPPING COST"]
[]
[]
[]
[null,null,"SPECIFICATION VERSION: March 22, 2024. "]