{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Munka1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Munka1","index":0,"n_rows":36,"n_cols":2,"rows_kept":36,"cut":false,"hidden":false,"merged":[[0,0,0,1],[78,0,78,1],[65,0,65,1],[1,0,1,1],[11,0,11,1],[22,0,22,1],[39,0,39,1],[51,0,51,1],[31,0,31,1],[2,0,2,1],[3,0,3,1]]}
["NECC PARTY rendezvénytechnikai specifikáció "]
[]
["Helyzín: Szeged Hungi"]
["Időpont: 2022.04.22"]
[]
["Hangtechnika","Mennyiség"]
["Sub hangsugárzó (min.146dB, 2x18\")",2]
["Szélessávú hangsugárzó (min.140dB, 1x12\", 1x3\")",2]
["Monitor hangsugárzó (min. 140dB, 1x12\", 1x3\")",6]
["Digitális keverőpult (min. 32csatorna, Yamaha,Avid,Digico)",1]
[]
["Fénytechnika"]
["Beam robotlámpa (min. 130W)",6]
["Spot robotlámpa (min. 120W LED v. Ezzel megegyező)",4]
["2-es LED-es sokkoló (min. 120W)",2]
["Stroboszkóp (min. 300W LED)",1]
["Ködgép (min. 1500W)",1]
["Fényvezérlő (min. 2univerzum)",1]
[]
["Videótechnika"]
["LEDfal 3,5m x 2m (min. P4,8)",1]
[]
["Színpadtechnika"]
["2m x 1m színpadlap állítható lábbal",4]
["10m alu truss (10m)",1]
["250kg-os emelő",2]
[]
["DJ technika"]
["Pioneer CDJ-2000NXS2",2]
["Pioneer DJM-900NXS2",1]
[]
["Személyzet"]
["Fénytechnikus",1]
["Hangtechnikus",1]
[]
["Szállítás",1]