{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Munka1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Munka1","index":0,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[1,1,1,4]]}
[]
[null,"Specifikáció - PB12778"]
[]
[null,"#","Cikkszám","Megnevezés","Mennyiség"]
[null,1,"779139-01","NI 9425 32-Ch 24 V, 7 us, Sinking DI Module",1]
[null,2,"779140-01","NI 9476 32-Ch 24 V, 500 us, Sourcing DO Module",1]
[null,3,"779892-02","NI 9871 4-Port RS422/RS485 Serial Module (Module Only)",5]
[null,4,"783376-01","NI 9149 8 Slot Ethernet Expansion chassis for C Series Modules",2]
[null,5,"196917-01","NI-9977 C Series Filler Module for Empty Slot",4]
[null,6,"784399-01","NI 9202 DSUB, 16-Ch, +/-10 V, 10 kS/s, 24-Bit, AI C Series Module",1]
[null,7,"781503-01","NI 9923 Front-mount terminal block for 37-pin D-Sub Modules",7]
[null,8,"780968-01","NI 9208, 24-bit current input module with DSub",4]