{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Műszaki leírás"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Műszaki leírás","index":0,"n_rows":12,"n_cols":3,"rows_kept":12,"cut":false,"hidden":false,"merged":[[0,0,0,2],[1,0,1,1]]}
["1. táblázat"]
["Előírt paraméterek, termékjellemzők, műszaki és minőségi elvárások, műszaki minimumkövetelmények",null,"Ajánlott paraméter"]
["Hidraulikus tetemszállító és emelő "]
["Szerkezet anyaga rozsdamentes Acél","Igen"]
["Szállító felület hosszúsága min. 2150 mm","Igen, kérjük megadni! "]
["Szállítófelület szélessége min. 700 mm","Igen, kérjük megadni! "]
["Terhelhetőség min. 200 kg","Igen, kérjük megadni! "]
["Min. 4 db gördíthető kerék, átmérőjük min. 120 mm","Igen, kérjük megadni! "]
["Állítható magasság lábpedál segítségével ","Igen"]
["Magasságállítás alsó végállása max. 330 mm","Igen, kérjük megadni! "]
["Magasságállítás felső végállása min. 1800 mm","Igen, kérjük megadni! "]
["Beépített digitális mérleg ","Opcionális "]